1.

[Brand New](https://computerstore.lk/product/corsair-ql140-rgb-140mm-pwm-dual-fan-kit-with-lighting-node-core/)

**CORSAIR QL140 RGB 140MM PWM DUAL FAN KIT WITH LIGHTING NODE CORE**

**LKR. 24,000**

* [**Description**](https://computerstore.lk/product/corsair-ql140-rgb-140mm-pwm-dual-fan-kit-with-lighting-node-core/#product-description)

|  |  |  |
| --- | --- | --- |
| Fan Size |  | 140mm x 25mm |
|  |  |  |
|  |  |  |
| Bearing Type |  | Hydraulic |
|  |  |  |
|  |  |  |
| Flow Type |  | Static Pressure |
|  |  |  |
|  |  |  |
| LED Color |  | RGB |
|  |  |  |
|  |  |  |
| Operating Voltage |  | 6V – 13.2V |
|  |  |  |
|  |  |  |
| PWM Control |  | YES |
|  |  |  |
|  |  |  |
| CORSAIR iCUE Compatibility |  | YES |
|  |  |  |
|  |  |  |
| Fan Model |  | QL Series |
|  |  |  |
|  |  |  |
| Weight |  | 0.469 |
|  |  |  |
|  |  |  |
| Package Quantity |  | 2 |
|  |  |  |
|  |  |  |
| Speed |  | 550 – 1250 ±10% RPM |
|  |  |  |
|  |  |  |
| Sound Level |  | 26 dBA |
|  |  |  |
|  |  |  |
| Power Draw |  | 0.30 A |
|  |  |  |
|  |  |  |
| Static Pressure |  | 1.4 mm-H2O |
|  |  |  |
|  |  |  |
| Adaptive Sync |  | RGB |
|  |  |  |
|  |  |  |
| Fan Airflow |  | 50.2 CFM |

2.

[Brand New](https://computerstore.lk/product/corsair-ql120-rgb-120mm-pwm-triple-fan-kit-with-lighting-node-core/)

##### CORSAIR QL120 RGB 120MM PWM TRIPLE FAN KIT WITH LIGHTING NODE CORE

##### LKR. 28,000

|  |  |  |
| --- | --- | --- |
| Fan Size |  | 120mm x 25mm |
|  |  |  |
| Bearing Type |  | Hydraulic |
|  |  |  |
| Flow Type |  | Static Pressure |
|  |  |  |
| LED Color |  | RGB |
|  |  |  |
| Operating Voltage |  | 6V – 13.2V |
|  |  |  |
| PWM Control |  | YES |
|  |  |  |
| CORSAIR iCUE Compatibility |  | YES |
|  |  |  |
| Fan Model |  | QL Series |
|  |  |  |
| Weight |  | 0.514 |
|  |  |  |
| Package Quantity |  | 3 |
|  |  |  |
| Speed |  | 525 – 1500 ±10% RPM |
|  |  |  |
| Sound Level |  | 26 dBA |
|  |  |  |
| Power Draw |  | 0.30 A |
|  |  |  |
| Static Pressure |  | 1.55 mm-H2O |
|  |  |  |
| Adaptive Sync |  | RGB |
|  |  |  |
| Fan Airflow |  | 41.8 CFM |

3.

##### CORSAIR H55 RGB 120MM LIQUID CPU COOLER

##### LKR. 19,000

* [**Specifications**](https://computerstore.lk/product/corsair-h55-rgb-120mm-liquid-cpu-cooler/#product-specifications)
* **» PART NUMBER:CW** - 9060052-WW
* **» LIGHTING:RGB**
* **» COOLING FAN:CPU Liquid Cooler**
* **» FAN SIZE:120mm**
* **» RADIATOR:Single Fan**
* [**Description**](https://computerstore.lk/product/corsair-h55-rgb-120mm-liquid-cpu-cooler/#product-description)

|  |  |  |
| --- | --- | --- |
| Cooling Warranty |  | 3 Year |
|  |  |  |
| Cold Plate Material |  | Copper |
|  |  |  |
| Radiator Material |  | Aluminum |
|  |  |  |
| PWM |  | Yes |
|  |  |  |
| CORSAIR iCUE Compatibility |  | Yes |
|  |  |  |
| Weight |  | 0.68 |
|  |  |  |
| Number of Fans |  | 1 |
|  |  |  |
| Cooling Socket Support |  | Intel 115x/1200 |
|  |  | Intel 2011/2066 |
|  |  | AMD AM4 |
|  |  |  |
| Lighting |  | RGB |
|  |  |  |
| Fan Model |  | SP Series |

4.

##### CORSAIR H150 RGB 360MM LIQUID CPU COOLER

##### LKR. 35,000

|  |  |  |
| --- | --- | --- |
| Cooling Warranty |  | 3 Year |
|  |  |  |
|  |  |  |
| Cold Plate Material |  | Copper |
|  |  |  |
|  |  |  |
| Radiator Material |  | Aluminum |
|  |  |  |
|  |  |  |
| PWM |  | Yes |
|  |  |  |
|  |  |  |
| CORSAIR iCUE Compatibility |  | Yes |
|  |  |  |
|  |  |  |
| Weight |  | 1.05 |
|  |  |  |
|  |  |  |
| Number of Fans |  | 3 |
|  |  |  |
|  |  |  |
| Cooling Socket Support |  | Intel 115x/1200 |
|  |  | Intel 2011/2066 |
|  |  | AMD AM4 |
|  |  |  |
|  |  |  |
| Lighting |  | RGB |
|  |  |  |
|  |  |  |
| Fan Model |  | SP Series |

5.

##### CORSAIR H100 RGB 240MM LIQUID CPU COOLER

##### LKR. 26,500

|  |  |  |
| --- | --- | --- |
| Cooling Warranty |  | 3 Year |
|  |  |  |
| Cold Plate Material |  | Copper |
|  |  |  |
| Radiator Material |  | Aluminum |
|  |  |  |
| PWM |  | Yes |
|  |  |  |
| CORSAIR iCUE Compatibility |  | Yes |
|  |  |  |
| Weight |  | 0.87 |
|  |  |  |
| Number of Fans |  | 2 |
|  |  |  |
| Cooling Socket Support |  | Intel 115x/1200 |
|  |  | Intel 2011/2066 |
|  |  | AMD AM4 |
|  |  |  |
| Lighting |  | RGB |
|  |  |  |
| Fan Model |  | SP Series |

6.

[Brand New](https://computerstore.lk/product/nzxt-kraken-z73-360mm-cpu-liquid-cooler/)

##### NZXT KRAKEN Z73 360MM CPU LIQUID COOLER

##### LKR. 70,000

* [**Specifications**](https://computerstore.lk/product/nzxt-kraken-z73-360mm-cpu-liquid-cooler/#product-specifications)
* **» PART NUMBER:RL** - KRZ73-01
* **» LIGHTING:RGB**
* **» COOLING FAN:CPU Liquid Cooler**
* **» FAN SIZE:120mm**
* **» RADIATOR:Dual Fan**
* [**Description**](https://computerstore.lk/product/nzxt-kraken-z73-360mm-cpu-liquid-cooler/#product-description)

|  |  |  |
| --- | --- | --- |
| Tech Specs |  |  |
|  |  |  |
|  |  |  |
| Cap |  |  |
|  |  |  |
| Diameter |  | 79mm |
|  |  |  |
| Height |  | 52mm |
|  |  |  |
| Material |  | Aluminum, Plastic |
|  |  |  |
| Fan Control |  | Yes |
|  |  |  |
| NZXT RGB Channel Connector |  | 1 |
|  |  |  |
| Rotation Orientation |  | Software adjustable Default, +90, +180, and -90 Degrees |
|  |  |  |
|  |  |  |
| LCD Display Panel |  |  |
|  |  |  |
| Active Area |  | 2.36″ (60mm) Diameter |
|  |  |  |
| Color |  | 24-bit True Color LCD |
|  |  |  |
| Resolution |  | 320 x 320px |
|  |  |  |
| Brightness |  | 650 cd/m² |
|  |  |  |
|  |  |  |
| Water Block |  |  |
|  |  |  |
| Material |  | Copper, Plastic |
|  |  |  |
|  |  |  |
| Pump |  |  |
|  |  |  |
| Motor Speed |  | 800 – 2,800 ± 300RPM |
|  |  |  |
| Power |  | 12V DC, 0.3A |
|  |  |  |
|  |  |  |
| Radiator |  |  |
|  |  |  |
| Dimensions |  | 121 x 394 x 27mm |
|  |  |  |
| Material |  | Aluminum |
|  |  |  |
|  |  |  |
| Tube |  |  |
|  |  |  |
| Length |  | 400mm |
|  |  |  |
| Material |  | Rubber with Nylon Sleeve |
|  |  |  |
|  |  |  |
| Fan Specs |  |  |
|  |  |  |
| Model |  | Aer P 120mm |
|  |  |  |
| Quantity |  | 3 |
|  |  |  |
| Speed |  | 500 – 2,000 ± 300RPM |
|  |  |  |
| Airflow |  | 18.28 – 73.11 CFM |
|  |  |  |
| Static Pressure |  | 0.18 – 2.93 mm-H₂O |
|  |  |  |
| Noise |  | 21 – 36 dBA |
|  |  |  |
| Fan Connector |  | 4-pin PWM |

##### 7.

##### NZXT KRAKEN Z53 240MM CPU LIQUID COOLER

* [**Specifications**](https://computerstore.lk/product/nzxt-kraken-z53-240mm-cpu-liquid-cooler/#product-specifications)
* **» PART NUMBER:RL** - KRZ53-01
* **» LIGHTING:RGB**
* **» COOLING FAN:CPU Liquid Cooler**
* **» FAN SIZE:120mm**
* **» RADIATOR:Dual Fan**

|  |  |  |
| --- | --- | --- |
| Tech Specs |  |  |
|  |  |  |
|  |  |  |
| Cap |  |  |
|  |  |  |
| Diameter |  | 79mm |
|  |  |  |
| Height |  | 52mm |
|  |  |  |
| Material |  | Aluminum, Plastic |
|  |  |  |
| Fan Control |  | Yes |
|  |  |  |
| NZXT RGB Channel Connector |  | 1 |
|  |  |  |
| Rotation Orientation |  | Software adjustable Default, +90, +180, and -90 Degrees |
|  |  |  |
|  |  |  |
| LCD Display Panel |  |  |
|  |  |  |
| Active Area |  | 2.36” (60mm) Diameter |
|  |  |  |
| Color |  | 24-bit True Color LCD |
|  |  |  |
| Resolution |  | 320 x 320px |
|  |  |  |
| Brightness |  | 650 cd/m² |
|  |  |  |
|  |  |  |
| Water Block |  |  |
|  |  |  |
| Material |  | Copper, Plastic |
|  |  |  |
|  |  |  |
| Pump |  |  |
|  |  |  |
| Motor Speed |  | 800 – 2,800 ± 300 RPM |
|  |  |  |
| Power |  | 12V DC, 0.3A |
|  |  |  |
|  |  |  |
| Radiator |  |  |
|  |  |  |
| Dimensions |  | 123 x 275 x 30mm |
|  |  |  |
| Material |  | Aluminum |
|  |  |  |
|  |  |  |
| Tube |  |  |
|  |  |  |
| Length |  | 400mm |
|  |  |  |
| Material |  | Rubber with Nylon Sleeve |
|  |  |  |
|  |  |  |
| Fan Specs |  |  |
|  |  |  |
| Model |  | Aer P120mm |
|  |  |  |
| Quantity |  | 2 |
|  |  |  |
| Speed |  | 500 – 2,000 ± 300RPM |
|  |  |  |
| Airflow |  | 18.28 – 73.11 CFM |
|  |  |  |
| Static Pressure |  | 0.18 – 2.93 mm-H₂O |
|  |  |  |
| Noise |  | 21 – 36 dBA |
|  |  |  |
| Fan Connector |  | 4-pin PWM |

##### 8.

##### ADATA XPG VENTO 120 ARGB CASE FAN

##### LKR. 4,300

* [**Specifications**](https://computerstore.lk/product/adata-xpg-vento-120-argb-case-fan/#product-specifications)
* **» BRAND:ADATA**
* **» PART NUMBER:75260103**
* **» STOCK AVAILABILITY:In stock**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| imensions | 120 x 120 x 25mm | |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Bearing Type | Rifle Bearing | |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Connector | 3-Pin |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Speed (RPM) | 1,200 RPM | |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Max Air Flow (CFM) | 45.3 |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Max Static Pressure (mmH2O) | 0.68 |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Noise Level (dBA) | 23dBA |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Rated Voltage | DC 12V |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Starting Voltage | DC 5V |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Operating Voltage | DC 5V – 12.6V | |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Rated Current | 0.16A (Max) | |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Power Dissipation | 1.92W |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Fan Protection | N/A |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| MTTF | At 40℃ 60,000 Hours | |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Cable Length | N/A |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Weight | N/A |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Note |  |  |  |  |
|  | VENTO 120 ARGB : | |  |  |
|  | LED Profiles : Addressable RGB LED | | | |
|  | LED Rated Voltage : DV 5V | | |  |
|  | LED Rated Current : 0.30A (max) | | | |
|  | LED Quantity : 9 | |  |  |

9.

##### RAIDMAX RF-S120LSR RED 120MM CASE FAN

##### LKR. 2,500

* [**Specifications**](https://computerstore.lk/product/raidmax-rf-s120lsr-red-120mm-case-fan/#product-specifications)
* **» BRAND:Raidmax**
* **» PART NUMBER:Raidmax RF** - S120LSR
* **» STOCK AVAILABILITY:In stock**

10.

##### CORSAIR AF140 LED BLUE QUIET EDITION HIGH AIRFLOW 140MM FAN

##### LKR. 4,000

Tech Spec

Fan Size – 140mm x 25mm

Fan Type – Quiet Edition

Flow Type – Airflow

LED Color – Blue

Operating Voltage – 7V – 12V

Airflow – 66.4 CFM

Static Pressure – .80 mmH20

Sound Level – 25.5 dBA

Speed – 1200 RPM

Power Draw – 0.23 A