1.

[Brand New](https://computerstore.lk/product/intel-pentium-gold-g6405-4m-cache-4-10-ghz-4-threads-2-cores-desktop-processor/)

**INTEL PENTIUM GOLD G6405 4M CACHE, 4.10 GHZ (4 THREADS, 2 CORES) DESKTOP PROCESSOR**

**LKR. 21,000**

**Availability: In Stock**

Specifications

* **» BRAND:Intel**
* **» PART NUMBER:BX80701G6405**
* **» PROCESSOR SERIES:Intel Pentium**
* [**Description**](https://computerstore.lk/product/intel-pentium-gold-g6405-4m-cache-4-10-ghz-4-threads-2-cores-desktop-processor/#product-description)

|  |  |
| --- | --- |
| Essentials |  |
| Product Collection | Intel® Pentium® Gold Processor Series |
| Code Name | Products formerly Comet Lake |
| Vertical Segment | Desktop |
| Processor Number | G6405 |
| Status | Launched |
| Launch Date | Q1’21 |
| Lithography | 14 nm |
| Use Conditions | PC/Client/Tablet |
| CPU Specifications |  |
| # of Cores | 2 |
| # of Threads | 4 |
| Processor Base Frequency | 4.10 GHz |
| Cache | 4 MB Intel® Smart Cache |
| Bus Speed | 8 GT/s |
| TDP | 58 W |
| Supplemental Information |  |
| Embedded Options Available | No |
| Datasheet | View now |
| Memory Specifications |  |
| Max Memory Size (dependent on memory type) | 128 GB |
| Memory Types | DDR4-2666 |
| Max # of Memory Channels | 2 |
| Max Memory Bandwidth | 41.6 GB/s |
| Processor Graphics |  |
| Processor Graphics ‡ | Intel® UHD Graphics 610 |
| Graphics Base Frequency | 350 MHz |
| Graphics Max Dynamic Frequency | 1.05 GHz |
| Graphics Video Max Memory | 64 GB |
| 4K Support | Yes, at 60Hz |
| Max Resolution (HDMI)‡ | 4096×2160@30Hz |
| Max Resolution (DP)‡ | 4096×2304@60Hz |
| Max Resolution (eDP – Integrated Flat Panel)‡ | 4096×2304@60Hz |
| DirectX\* Support | 12 |
| OpenGL\* Support | 4.5 |
| Intel® Quick Sync Video | Yes |
| Intel® InTru™ 3D Technology | Yes |
| Intel® Clear Video HD Technology | Yes |
| Intel® Clear Video Technology | Yes |
| # of Displays Supported ‡ | 3 |
| Device ID | 0x9BA8 |
| Expansion Options |  |
| Scalability | 1S Only |
| PCI Express Revision | 3 |
| PCI Express Configurations ‡ | Up to 1×16, 2×8, 1×8+2×4 |
| Max # of PCI Express Lanes | 16 |

2.

[Brand New](https://computerstore.lk/product/corsair-rm850-850-watt-80-plus-gold-certified-fully-modular-power-supply/)

##### CORSAIR RM850 – 850 WATT 80 PLUS GOLD CERTIFIED FULLY MODULAR POWER SUPPLY

##### LKR. 36,000

* [**Description**](https://computerstore.lk/product/corsair-rm850-850-watt-80-plus-gold-certified-fully-modular-power-supply/#product-description)

|  |  |  |
| --- | --- | --- |
| Adjustable Single/Multi 12V Rail |  | No |
| ATX Connector |  | 1 |
| ATX12V Version |  | v2.52 |
| Continuous output rated temperature C |  | 50°C |
| Continuous power W |  | 850 Watts |
| Fan bearing technology |  | Rifle Bearing |
| Fan size mm |  | 135mm |
| MTBF hours |  | 100,000 hours |
| Multi-GPU ready |  | Yes |
| Warranty |  | Three Years |
| 80 PLUS Efficiency |  | Gold |
| PSU Form Factor |  | ATX |
| iCUE Compatibility |  | No |
| Zero RPM Mode |  | Yes |
| Cable Type |  | Low-Profile, All Black |
| Dimensions |  | 150mm x 86mm x 160mm |
| EPS12V Connector |  | 2 |
| EPS12V Version |  | v2.92 |
| Floppy Connector |  | 0 |
| Modular |  | Fully |
| PCIe Connector |  | 6 |
| SATA Connector |  | 12 |
| PATA Connector |  | 4 |
| Modern Standby Compatible |  | Yes |

3.

[Brand New](https://computerstore.lk/product/corsair-rm750-750-watt-80-plus-gold-certified-fully-modular-power-supply/)

##### CORSAIR RM750 – 750 WATT 80 PLUS GOLD CERTIFIED FULLY MODULAR POWER SUPPLY

##### LKR. 30,500

* [**Description**](https://computerstore.lk/product/corsair-rm750-750-watt-80-plus-gold-certified-fully-modular-power-supply/#product-description)

|  |  |
| --- | --- |
| ATX Connector | 1 |
| Adjustable Single/Multi 12V Rail | No |
| ATX12V Version | v2.52 |
| Continuous output rated temperature C | 50°C |
| Continuous power W | 750 Watts |
| Fan bearing technology | Rifle Bearing |
| Fan size mm | 135mm |
| MTBF hours | 100,000 hours |
| Multi-GPU ready | Yes |
| Warranty | Three Years |
| 80 PLUS Efficiency | Gold |
| PSU Form Factor | ATX |
| Zero RPM Mode | Yes |
| iCUE Compatibility | No |
| Cable Type | Low-Profile, All Black |
| Dimensions | 150mm x 86mm x 160mm |
| EPS12V Connector | 2 |
| EPS12V Version | v2.92 |
| Floppy Connector | 0 |
| Modular | Fully |
| PCIe Connector | 6 |
| SATA Connector | 10 |
| PATA Connector | 4 |
| Modern Standby Compatible | Yes |

4.

[Brand New](https://computerstore.lk/product/corsair-rm1000x-80-plus-gold-certified-power-supply/)

##### CORSAIR RM1000X 80 PLUS GOLD CERTIFIED POWER SUPPLY

##### LKR. 51,500

* [**Description**](https://computerstore.lk/product/corsair-rm1000x-80-plus-gold-certified-power-supply/#product-description)
* ATX Connector – 1
* Ability to toggle singlemultiple 12V rails – No
* ATX12V Version – v2.4
* Continuous output rated temperature C – 50°C
* Continuous power W – 1000 Watts
* Corsair Link Support – No
* Fan bearing technology – Rifle
* Fan size mm – 135mm
* MTBF hours – 100,000 hours
* Multi-GPU ready – YES
* Power – 1000 Watts
* 80 PLUS Efficiency – Gold
* PSU Form Factor – ATX
* Zero RPM Mode – Yes
* Cable Type – Sleeved and Flat Black Cables
* C-Link Ready – No
* Dimensions – 150mm x 86mm x 180mm
* EPS Connector – 2
* Floppy Connector – 1
* Modular – Fully
* PCI-E Connector – 8
* Plug Type – NA
* SATA Connector – 11

5.

##### RAIDMAX RX-500AF-V BRONZE CERTIFIED POWER SUPPLY

##### LKR. 9,000

* [**Description**](https://computerstore.lk/product/raidmax-rx-500af-v-bronze-certified-power-supply-2/#product-description)
* » BRAND:Raidmax
* » PART NUMBER:RX-500AF-V Bronze
* » ENERGY EFFICIENCY:80 Plus Bronze
* » MODULARITY:Standard

6.

[Brand New](https://computerstore.lk/product/raidmax-rx-500ac-vr-rgb-500-watt-80-plus-bronze-certified-power-supply/)

##### RAIDMAX RX-500AC-VR RGB – 500 WATT 80 PLUS BRONZE CERTIFIED POWER SUPPLY

##### LKR. 10,500

Specifications

* **» BRAND:Raidmax**
* **» PART NUMBER:RX** - 500AC-VR RGB
* **» ENERGY EFFICIENCY:80 Plus Bronze**

7.

##### RAIDMAX RX-700AC-VR RGB – 500 WATT 80 PLUS BRONZE CERTIFIED POWER SUPPLY

##### LKR. 13,000

[Brand New](https://computerstore.lk/product/raidmax-rx-700ac-vr-rgb-500-watt-80-plus-bronze-certified-power-supply/)

**RAIDMAX RX-700AC-VR RGB – 500 WATT 80 PLUS BRONZE CERTIFIED POWER SUPPLY**

**LKR. 13,000**

**Availability: In Stock**

Specifications

* **» BRAND:Raidmax**
* **» PART NUMBER:RX** - 700AC-VR RGB
* **» ENERGY EFFICIENCY:80 Plus Bronze**

8.

[Brand New](https://computerstore.lk/product/nzxt-c650-80-plus-gold-uk-power-supply/)

##### NZXT C650 80 PLUS GOLD (UK) POWER SUPPLY

##### LKR. 27,000

* [**Specifications**](https://computerstore.lk/product/nzxt-c650-80-plus-gold-uk-power-supply/#product-specifications)
* **» BRAND:**
* **NZXT**
* **» PART NUMBER:**
* **NP** - C650M-UK
* **» ENERGY EFFICIENCY:**
* **80 Plus Gold**
* **» MODULARITY:**
* **Fully Modular**
* [**Description**](https://computerstore.lk/product/nzxt-c650-80-plus-gold-uk-power-supply/#product-description)
* Steel, PCB, and plastic
* 150 x 150 x 86mm
* 100-240Vac, 8-4A, 50-60Hz
* Connectors:
* 1x 24-pin ATX power
* 1x (610mm, Nylon sleeving)
* 1x 4+4-pin CPU power
* 1x (650mm, Nylon sleeving)
* 2x PCIe (6+2 pin)
* 1x (675+75mm, Nylon sleeving)
* 8x Sata
* 2x (500 + 100 + 100 + 100mm)
* 3x Peripherals
* 1x (500 + 100 +100mm)
* 10 Year Warranty

9.

[Brand New](https://computerstore.lk/product/corsair-rm650-650-watt-80-plus-gold-certified-fully-modular-power-supply/)

**CORSAIR RM650 – 650 WATT 80 PLUS GOLD CERTIFIED FULLY MODULAR POWER SUPPLY**

**LKR. 25,000**

**Availability: In Stock**

Specifications

* **ENERGY EFFICIENCY**
* **80 Plus Gold**

**DESCRIPTION :**

|  |  |  |
| --- | --- | --- |
| Adjustable Single/Multi 12V Rail |  | No |
|  |  |  |
|  |  |  |
| ATX Connector |  | 1 |
|  |  |  |
|  |  |  |
| ATX12V Version |  | v2.4 |
|  |  |  |
|  |  |  |
| Continuous output rated temperature C |  | 40°C |
|  |  |  |
|  |  |  |
| Continuous power W |  | 650 Watts |
|  |  |  |
|  |  |  |
| Fan bearing technology |  | Rifled |
|  |  |  |
|  |  |  |
| Fan size mm |  | 140mm |
|  |  |  |
|  |  |  |
| MTBF hours |  | 100,000 hours |
|  |  |  |
|  |  |  |
| Multi-GPU ready |  | YES |
|  |  |  |
|  |  |  |
| Power |  | 650 Watts |
|  |  |  |
|  |  |  |
| Warranty |  | Three years |
|  |  |  |
|  |  |  |
| 80 PLUS Efficiency |  | Gold |
|  |  |  |
|  |  |  |
| PSU Form Factor |  | ATX |
|  |  |  |
|  |  |  |
| Zero RPM Mode |  | Yes |
|  |  |  |
|  |  |  |
| Cable Type |  | Low-Profile, All Black |
|  |  |  |
|  |  |  |
| C-Link Ready |  | No |
|  |  |  |
|  |  |  |
| Dimensions |  | 150mm x 86mm x 160mm |
|  |  |  |
|  |  |  |
| EPS12V Connector |  | 1 |
|  |  |  |
|  |  |  |
| Floppy Connector |  | 2 |
|  |  |  |
|  |  |  |
| Modular |  | Fully |
|  |  |  |
|  |  |  |
| PCIe Connector |  | 4 |
|  |  |  |
|  |  |  |
| Plug Type |  | NA |
|  |  |  |

10.

[Brand New](https://computerstore.lk/product/raidmax-rx-300xt-80-plus-standard-power-supply/)

**Raidmax RX-300XT 80 Plus Standard Power Supply**

**LKR. 5,000**

» BRAND: Raidmax  
» PART NUMBER: RX-300XT  
» ENERGY EFFICIENCY: 80 Plus  
» MODULARITY: Standard

**Availability: In Stock**

Specifications

* **M/b 20+4 PIN – 1**
* **CPU 4+4 PIN – 1**
* **PCI** - E 6+2 PIN –